
samples 说明：
AppEncD3D11.exe: 		从本地文件读取YUV数据进行编码，码流写入指定的文件。
AppEncD3D11Perf.exe: 	衡量FPS中的编码性能(一次性读入文件，所以YUV文件不宜过大)，码流不写入文件。
AppEncDDA.exe: 			捕获桌面，并对捕获的图像进行编码 (用于virtual display场景)，码流写入文件 DDABitStream_x_x.h264。


samples使用方法:  
1. 准备一个 NV12 文件(用于 AppEncD3D11.exe 或 AppEncD3D11Perf.exe)
2. 打开命令提示符，执行如下命令: 
	AppEncD3D11.exe -i 1920x1080_nv12.yuv -s 1920x1080 -src_fmt nv12 -bf 0 -rc cqp -constqp 20 -fps 25 -gop 30 -frames 100 -o out.h264
	或
	AppEncD3D11Perf.exe -i 1920x1080_nv12.yuv -s 1920x1080 -src_fmt nv12 -bf 0 -rc cqp -constqp 20 -fps 25 -gop 30 -frames 50000 -o out-cqp.h264
	或
	AppEncDDA.exe (用于virtual display场景)
3. 参数说明：
	AppEncD3D11.exe/AppEncD3D11Perf.exe Options:
	-i           Input file path
	-o           Output file path
	-s           Input resolution in this form: WxH
	-src_fmt     input file pixel format(nv12, bgra)
	-frames      encode frame number
	-profile     H264: auto baseline main high
	-fps         Frame rate
	-gop         Length of GOP (Group of Pictures)
	-bf          Number of consecutive B-frames
	-rc          Rate control mode: cqp cbr
	-bitrate     Average bit rate, can be in unit of 1, K, M
	-constqp     QP value for cqp rate control mode
	
	AppEncDDA.exe Options:
	-frames      encode frame number